COMMAND FLOW SEQUENCE

The flow of commands follows a logical diagnostic and messaging sequence:

AT → AT+CSQ → AT+CMGF=1 → AT+CMGS → AT+CMGR

This sequence checks modem status, signal strength, sets SMS mode, sends an SMS, and then reads it.