AT Command Sequence

Command Log and Description

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Step | Command | Expected Response | Actual Response | Notes |
| 1 | AT | OK | OK | Modem is responsive |
| 2 | AT+CSQ? | +CSQ: <rssi>,<ber> OK | ERROR | Command not supported in emulator |
| 3 | AT+CSQ | +CSQ: <rssi>,<ber> OK | +CSQ: 21,0 OK | Signal strength is good (RSSI=21) |
| 4 | AT+CMGF=1 | OK | OK | Text mode enabled |
| 5 | AT+CMGS="1234567890" HELLO + Ctrl+Z | +CMGS: 1 OK | +CMGS: 1 OK | SMS sent and stored at index 1 |
| 6 | AT+CMGR=1 | +CMGR: ... message\nOK | ERROR | Read failed; likely unsupported |